Meusburger Georg GmbH & Co KG

Kesselstr. 42, 6960 Wolfurt, Austria

**NEW from Meusburger – Ejectors for longer service life**

**The new HSS ejector pins and DLC coated blade ejector pins with extra long blade from Meusburger guarantee long life and minimal wear. The use of high-speed steel and diamond-like carbon coating results in longer maintenance intervals and reduced downtimes. The two high-quality ejectors are as usual with Meusburger, available from stock.**

**HSS ejector pins**

When using HSS ejector pins, moulds can be operated at higher temperatures due to the pins' excellent high-temperature resistance. In addition, minimal wear is guaranteed through their hardness of ~64HRC.

**DLC coated blade ejector pins with extra long blade**

The DLC coated blade ejectors assure highest precision and longest service life through the best sliding properties. Excellent corrosion resistance is in addition to their usability in cleanrooms a further advantage of the DLC coated ejectors. Available with 2 or 4 angle radii, the blade ejectors are ideally suited for the installation in EDMed apertures.

**Picture credits:** Photo (Meusburger)

**Caption:** New ejectors from Meusburger ensure longer service life



**Meusburger – Setting Standards**

Meusburger is the **leading manufacturer of high-precision standard parts**. More than 17,000 customers all over the world make use of the numerous advantages of standardisation and benefit from the company's **over 50 years of experience** in working with steel. Offering an extensive **range of standard parts**, combined with **high-grade products in the field of workshop equipment**, Meusburger is the **reliable global partner** for **making dies, moulds, jigs and fixtures.**

**Further information:**

|  |
| --- |
| Meusburger Georg GmbH & Co KGCommunication / Public relationsPhone: 0043 (0) 5574 6706-0Email address: presse@meusburger.com<http://www.meusburger.com/press-releases> |